{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":258,"n_cols":9,"rows_kept":258,"flags":["formulas_cached_only"]}
["单位名称","所属实验室或成员单位","所属功能平台","所属领域","名称","厂商及型号","国别","性能参数","服务功能"]
["中国家用电器研究院","零部件一部","电子信息系统","电子信息","加热管加速寿命试验机","RG-H-803","中国","电源0-600V（3个），0-1200V（1个），测温仪100-1000℃，","加热管加速寿命试验"]
["中国家用电器研究院","零部件部-灯具电机室","电子、电器产品","电子信息","灯具耐久实验室","中家智锐，恒温实验室","中国","15～40℃，±1℃","灯具等产品耐久测试"]
["中国家用电器研究院","零部件部-灯具电机室","电子、电器产品","电子信息","灯具综合实验室","中家智锐，灯具检测环境室","中国","15～40℃，±1℃","灯具等产品耐久测试"]
["中国家用电器研究院","系统可靠性测试中心","电子信息系统","电子信息","快温变环境试验箱","C7-800/15","中国","-70℃~180℃","温度、湿度环境试验"]
["中国家用电器研究院","系统可靠性测试中心","电子信息系统","电子信息","万能材料试验机","2336.0","美国","0~5000N","拉伸、压缩性能测试"]
["中国家用电器研究院","消费电子及EMC检测中心-EMC检测部","电子信息系统","电子信息","传导抗扰度综合测试主机","TESEQ   NSG4070C-80","瑞士","150kHz-230MHz 80W","传导抗扰度测试"]
["中国家用电器研究院","消费电子及EMC检测中心-EMC检测部","电子信息系统","电子信息","单相交流电压源","EM TEST   ACS 500N6","瑞士","输出功率最大6000VA，频率范围10Hz-80Hz","谐波闪烁测试"]
["中国家用电器研究院","消费电子及EMC检测中心-EMC检测部","电子信息系统","电子信息","单相谐波闪烁分析仪","EM TEST   DPA 500N","瑞士","1-50次谐波测试；Pst 和 Plt 精度优于5%；dmax，dc，dt精度优于0.15%","谐波闪烁测试"]
["中国家用电器研究院","消费电子及EMC检测中心-EMC检测部","电子信息系统","电子信息","屏蔽室","ETS-Lindgren   S81","美国","7m*4m*3.5m","传导骚扰测试"]
["中国家用电器研究院","后勤保障部","电子信息系统","电子信息","空调机组","/","中国","220V 50Hz","提供室内稳定工作环境温度"]
["中国家用电器研究院","零部件一部","电子信息系统","电子信息","电容器耐久性试验台","CBE-6800D","中国","交流电压：100-600V，交流电流：5-25A，直流电压：1-4.5kV,短路电流：5-50mA","电容器耐久性试验"]
["中国家用电器研究院","计量事业部","电子信息系统","电子信息","交流标准电压/电流源","220.0","中国","220V 50Hz","提供稳态电压稳态电源"]
["中国家用电器研究院","计量事业部","电子信息系统","电子信息","制冷恒温槽","9190A-C-256","中国","220V 50Hz","制冷系统具有过热、过电流保护，控制系统具有超温鸣叫报警，可设定上下限超温报警温度，超温时可自动切断负载"]
["中国家用电器研究院","健康家电分析测试中心","节能","能源环保","待机能耗综合测试系统","ATR Sysrem SP","中国","220V 50Hz","测试待机能耗"]
["中国家用电器研究院","健康家电分析测试中心","节能","能源环保","数字化白度测试系统","DWTS-1","中国","零点漂移≤0.1，示值漂移≤0.1，工作环境温度0-40℃，相对湿度0-85%","测量白度光学系统的光谱功率分布"]
["中国家用电器研究院","电子产品检查部-EMC二部","电子信息系统","电子信息","EMI测量接收机测试设备","","美国","3Hz-44GHz","传导、辐射骚扰测试"]
["中国家用电器研究院","零部件二部","电子信息系统","电子信息","光辐射安全测定系统","杭州远方 OST-500","中国","波长 200nm至3000nm","照明器具、显示屏等光生物安全（蓝光危害、光生物、光辐射等）"]
["中国家用电器研究院","信息服务平台","电子信息系统","电子信息","存储设备","DELL SCv2000","中国","220V 50Hz","存储实验室数据"]
["中国家用电器研究院","健康家电分析测试中心","节能","能源环保","步入式恒温恒湿箱","HTP420","中国","220V 50Hz","本设备适用于各类电工电子产品及其他产品、渐变、交变、湿热变化等环境模拟可靠性试验"]
["中国家用电器研究院","测试技术研究所","电子信息系统","电子信息","噪声振动测试系统升级改造","CHE2012-12/08 北京中家智锐科技有限公司","中国","220V 50Hz","噪声振动测试"]
["中国家用电器研究院","健康家电分析测试中心","节能","能源环保","质构仪","TMS-Pro","中国","力量感应元的选择：2、5、10、30、50、100Kg，距离行程：0~330mm（根据需要增减），数据采集速度：最大500个样/秒，以软件为准。电源：100-250VAC 50-60Hz","可以准确检测食品样品随时间变化的位置和重量从而给出样品的物性特征。力的数据存数在表格里并且曲线显示"]
["中国家用电器研究院","零部件一部","电子、电器产品","电子信息","温控器耐久性试验机","瑞格电子科技有限公司RG-E80210","中国","20-100℃；55-300℃","低温箱；高温箱"]
["中国家用电器研究院","零部件一部","电子、电器产品","电子信息","电动水阀耐久性试验机","瑞格电子科技有限公司RG-W80201","中国","50V-300V;12V-60V;0-1.6MPa;","交流电压；直流电压；压力"]
["中国家用电器研究院","材料分析中心","","新材料","超离心研磨仪","ZM200","","6000 - 18000r/min",""]
["中国家用电器研究院","材料分析中心","","新材料","气相色谱仪","K0733B733700000","","检出限:9.3×10-12g/s",""]
["中国家用电器研究院","材料分析中心","","新材料","原子荧光仪","sk-盛析","","As Sb Bi Pb Sn Te Se＜0.01ng/mL,Zn＜1.0,Ge＜0.05 Cd Hg＜0.001,检出限(k=3)：0.004ng[砷]",""]
["中国家用电器研究院","材料分析中心","","新材料","原子吸收分光光度计（火焰）","240FS AA","","检出限(k=3)：0.010μg/mL[铜]",""]
["中国家用电器研究院","材料分析中心","","新材料","原子吸收分光光度计（石墨炉）","240Z AA","","检出限(k=3)：0.1pg[镉]",""]
["中国家用电器研究院","材料分析中心","","新材料","热重分析仪","TG 209 F3","","室温~1000℃，0.001℃/min~100℃/min，0~2g,0.1μg",""]
["中国家用电器研究院","材料分析中心","","新材料","差示扫描量热仪","DSC 200 F3","","﹣170~600/700℃,0.001°C/min~100°C/min",""]
["中国家用电器研究院","材料分析中心","","新材料","紫外-可见光分光光度计UV-VIS","Heλiosα","","190-1100nm,示值误差：(-0.6~0.8)nm",""]
["中国家用电器研究院","材料分析中心","","新材料","微波消解器","Mars5","","﹣40~300，2450MHz",""]
["中国家用电器研究院","材料分析中心","","新材料","气相色谱－质谱联用仪(GC-MS)","TraceGC/DSQ","","1-1050amu,不确定度U=3%,k=2",""]
["中国家用电器研究院","材料分析中心","","新材料","电感耦合等离子体发射光谱仪(ICP","IRIS Intrepid II XSP","","165-1000 nm,检出限：0.0006mg/L[钡]",""]
["中国家用电器研究院","材料分析中心","","新材料","红外光谱仪","Nicolet6700","","波长27000~15 cm-1，分辨率0.09 cm-1",""]
["中国家用电器研究院","材料分析中心","","新材料","红外光谱仪","Nicolet is5","","波长8000-350 cm-1，分辨率0.8cm-1",""]
["中国家用电器研究院","材料分析中心","","新材料","热重分析仪","Q500","","室温~1000℃，准确度±1℃，称重精度±0.01%",""]
["中国家用电器研究院","材料分析中心","","新材料","差示扫描量热仪","Q20","","﹣180~725℃，± 0.05 ℃",""]
["中国家用电器研究院","材料分析中心","","新材料","gc-ms自动进样器","/","","/",""]
["中国家用电器研究院","材料分析中心","","新材料","能量色散X荧光光谱仪","EDX-LE","","13Al-92U,Cl",""]
["中国家用电器研究院","EMC一部","","电子信息","EA电源","PS 9750-60","","输出电压：0-750V；输出电流：0-60A；输出功率：0-15kW",""]
["中国家用电器研究院","理化分析室","","新材料","能量色散X荧光光谱仪","EDX-LE","","13Al-92U,Cl",""]
["中国家用电器研究院","通用部","","电子信息","噪声振动测试分析系统（室内测试）","CHE2012-12","","频率：20Hz～20kHz； 本底噪声：<10dBA；A计权频率响应见校准结果。8通道",""]
["中国家用电器研究院","通用部","","电子信息","噪声振动测试分析系统（室外测试）","CHE2012-12","","频率：20Hz～20kHz； 本底噪声：<10dBA；A计权频率响应见校准结果。12通道",""]
["中国家用电器研究院","通用部","","电子信息","静音测试系统","2690和4179","","频率：20Hz～20kHz； 本底噪声：-1.95dBA；\n20Hz～250Hz, U=0.5dB,k=2\n500Hz～1kHz, U=0.3dB,k=2\n2kHz～20kHz, U=0.5dB,k=2",""]
["中国家用电器研究院","系统可靠性测试中心","","新材料","系统金相显微镜","BX51M","","220V AC  50Hz",""]
["中国家用电器研究院","测试技术研究所","","新材料","差热-热重同步分析仪","DTG-60","","-500mg~500mg",""]
["中国家用电器研究院","系统可靠性测试中心","","新材料","可编程交流电源","61511","","交流部分：150V 量程：输入380V输出110V，负载32A，300V量程：输入380V输出220V，负载16A  频率1500Hz",""]
["中国家用电器研究院","系统可靠性测试中心","","新材料","高加速寿命试验箱","Ryphoon-4.0+","","升降温速率≥60℃/min；温度极限值低温-100℃，高温200℃；振动量级：Z轴≥60GRMS，X、Y轴大于等于30GRMS；频率范围0-10000HZ。振动量级均匀度≤40%",""]
["中国家用电器研究院","测试技术研究所","","新材料","总有机碳分析仪","TOC-V WP","","(0-300)ppb",""]
["中国家用电器研究院","大家电一部","","新材料","空调热舒适性测试实验室","","","温控表50摄氏度/湿度以表/热电偶/电参数(电压V电流A频率Hz)",""]
["中国家用电器研究院","测试技术研究所","","新材料","高效液相色谱仪","LC-20A","","紫外检测器：基线噪声≤5×10-4AU；基线漂移：≤5×10-3AU/30min；最小检测浓度：≤5×10-8g/mL萘-甲醇溶液；波长重复性：≤2nm。荧光检测器：基线噪声≤5×10-4FU；基线漂移：≤5×10-3FU/30min；最小检测浓度：≤5×10-9g/mL萘-甲醇溶液；波长重复性：≤2nm",""]
["中国家用电器研究院","理化分析室","","新材料","热重分析仪","TG209F3","","室温~1000℃，0.001℃/min~100℃/min，0~2g,0.1μg",""]
["中国家用电器研究院","理化分析室","","新材料","差示扫描量热仪","DSC214","","﹣85/﹣70~600℃,0.001 K/min~500 K/min,750 Mw",""]
["中国家用电器研究院","理化分析室","","新材料","热重分析仪","TG209F3","","室温~1000℃，0.001℃/min~100℃/min，0~2g,0.1μg",""]
["中国家用电器研究院","零部件一部","","电子信息","开关寿命试验机","YH-8815CSC","","往复频率（15次/分、30次/分）",""]
["中国家用电器研究院","测试技术研究所","","新材料","离子色谱仪","881","","0.4ppm-50ppm",""]
["中国家用电器研究院","","","新材料","雷击浪涌抗扰度测试系统","特测","瑞士","",""]
["中国家用电器研究院","","","新材料","快速瞬变脉冲群抗绕度测试系统","特测","瑞士","",""]
["中国家用电器研究院","","","新材料","静电放电抗绕度测试系统","特测","瑞士","",""]
["中国家用电器研究院","","","新材料","工频磁场抗扰度设备","EMTESTS","","",""]
["中国家用电器研究院","","","新材料","屏蔽室","ETS","","",""]
["中国家用电器研究院","","","新材料","暗室配套设备","RS/特测","瑞士","",""]
["中国家用电器研究院","","","新材料","半波暗室","嘉善法兰克尼亚电磁兼容有限公司","德国","",""]
["中国家用电器研究院","","","新材料","摆管淋雨试验系统","锐铧","国内","",""]
["中国家用电器研究院","","","新材料","噪声测试设备","BK","国内","",""]
["中国家用电器研究院","","","新材料","冰箱压缩机量热计","大学热学","日本","",""]
["中国家用电器研究院","","","新材料","5匹工况调节精密级半消声室","院噪声课题组","国内","",""]
["中国家用电器研究院","","","新材料","人工气候环境试验室","工程部","国内","",""]
["中国家用电器研究院","","","新材料","空调压缩机寿命,停开","工程部","国内","4工位",""]
["中国家用电器研究院","","","新材料","压缩机耐压试验装置","工程部","国内","",""]
["中国家用电器研究院","","","新材料","R134a冰箱压缩机毛细管堵塞试验台","工程部","国内","",""]
["中国家用电器研究院","","","新材料","压缩机堵转试验台及控制系统","工程部","国内","",""]
["中国家用电器研究院","","","新材料","空调压缩机非正常试验装置","工程部","国内","",""]
["中国家用电器研究院","","","新材料","冰箱压缩机非正常试验台","工程部","国内","",""]
["中国家用电器研究院","","","新材料","空调压缩机量热计","大西热学","日本","",""]
["中国家用电器研究院","","","新材料","分断系统(一期限定短路实验装置)","苏州安泰变压器厂","国内","",""]
["中国家用电器研究院","","","新材料","开关耐久性试验装置","东莞锐铧","国内","",""]
["中国家用电器研究院","","","新材料","控制器类产品耐久性试验台","青岛科通","国内","",""]
["中国家用电器研究院","","","新材料","电容器测试台","广州微仪电子","国内","",""]
["中国家用电器研究院","","","新材料","台、吊扇试验室","广州市先河技术工程有限公司","国内","",""]
["中国家用电器研究院","","","新材料","吸油烟机气味降低度试验装置","青岛科通","国内","",""]
["中国家用电器研究院","","","新材料","室内加热器试验室","青岛科通","国内","",""]
["中国家用电器研究院","","","新材料","换气扇性能试验室(A、C型)","广州市先河技术工程有限公司","国内","",""]
["中国家用电器研究院","","","新材料","热水器性能试验室","青岛科通","国内","",""]
["中国家用电器研究院","","","新材料","吸油烟机空气性能试验装置(B型)","工程部","国内","",""]
["中国家用电器研究院","","","新材料","吸油烟机油脂分离度试验装置","工程部","国内","",""]
["中国家用电器研究院","","","新材料","脉冲压力测试仪","工程部","国内","5MPa",""]
["中国家用电器研究院","","","新材料","可燃制冷剂模拟泄漏装置(自动控制)","工程部","国内","",""]
["中国家用电器研究院","","","新材料","洗衣机安全试验台","工程部","国内","8台位","清洁器具检测"]
["中国家用电器研究院","","","新材料","焓差空调测试室","工程部","国内","30HP","制冷器具检测"]
["中国家用电器研究院","","","新材料","空调焓差试验室","工程部","国内","5HP","制冷器具检测"]
["中国家用电器研究院","","","新材料","食品冷柜型式试验室","工程部","国内","四台位","制冷器具检测"]
["中国家用电器研究院","","","新材料","冰箱性能试验室","工程部","国内","六台位","制冷器具检测"]
["中国家用电器研究院","","","新材料","空调热平衡试验室","大西热学","日本","3HP","制冷器具检测"]
["中国家用电器研究院","","","新材料","空调焓差试验室","大西热学","日本","5HP","制冷器具检测"]
["中国家用电器研究院","","","新材料","冰箱试验室","佐竹冷热","日本","六台位","制冷器具检测"]
["中国家用电器研究院","","","新材料","气相色谱仪","北京绿绵科技赛默traceultra,traceultra","日本","","六种有毒有害物质检测"]
["中国家用电器研究院","","","新材料","原子荧光仪","北京金正索坤公司sk-盛析,sk-盛析","日本","","清洁器具检测"]
["中国家用电器研究院","","","新材料","原子吸收分光光度计","安捷伦科技公司240FS+240Z,240FS+240Z","日本","","清洁器具检测"]
["中国家用电器研究院","","","新材料","热重分析仪","耐驰科学仪器商贸（上海）有限公司北京分公司TG209F3,TG209F3","日本","","清洁器具检测"]
["中国家用电器研究院","","","新材料","差示扫描量热仪","耐驰科学仪器商贸（上海）有限公司北京分公司DSC200F3,DSC200F3","日本","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","分光光度计","北京博通达科技有限公司Datacolor600,Datacolor600","日本","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","连续波模拟器","瑞士EMTEST公司CWS500N1,CWS500N1","瑞士","0.1MHz-300MHz","电磁兼容检测"]
["中国家用电器研究院","","","新材料","紫外-可见光分光光度计（UV-VIS","美国THERMO公司Heiosa,Heiosa","美国","","六种有毒有害物质检测"]
["中国家用电器研究院","","","新材料","微波消解器","美国GEM公司Mars5,Mars5","美国","","六种有毒有害物质检测"]
["中国家用电器研究院","","","新材料","气相色谱－质谱联用仪(GC-MS)","美国THERMO公司TraceDSQ,TraceDSQ","美国","","压缩机产品检测"]
["中国家用电器研究院","","","新材料","电感耦合等离子体发射光谱仪(ICP","美国THERMO公司IRISIntrepi,IRISIntrepi","美国","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","断续骚扰（喀呖声）测量仪","SCHAFFNER公司DIA1512D,DIA1512D","日本","150k-30MHz","电磁兼容检测"]
["中国家用电器研究院","","","新材料","谐波闪烁测试系统","美国加利福尼亚仪器有限公司MXCTS-45,MXCTS-45","美国","单相≤150A三相≤50A","电磁兼容检测"]
["中国家用电器研究院","","","新材料","模拟灯","德国SCHWARZBECK","德国","LN系列、RS系列","电磁兼容检测"]
["中国家用电器研究院","","","新材料","质谱仪","美国","美国","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","闭孔率测试仪","美国麦克仪器公司","美国","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","屏蔽室","美国LINDGREN公司CellTYPE,CellTYPE","美国","14kHz-18GHz屏蔽效能>60dB","电磁兼容检测"]
["中国家用电器研究院","","","新材料","连续波模拟器","瑞士EMTEST公司CWS500,CWS500","瑞士","0.1MHz-300MHz","电磁兼容检测"]
["中国家用电器研究院","","","新材料","快速脉冲串发生器","瑞士SCHAFFNER公司NSG2025-4,NSG2025-4","瑞士","250V-4kV","电磁兼容检测"]
["中国家用电器研究院","","","新材料","静电放电模拟器","瑞士SCHAFFNER公司NSG435,NSG435","瑞士","2kV-16.5kV","电磁兼容检测"]
["中国家用电器研究院","","","新材料","断续干扰分析仪","英国Chase公司DIA1512B,DIA1512B","英国","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","谐波和闪烁测试装置","瑞士SCHAFFNER公司2000,2000","瑞士","","电磁兼容检测"]
["中国家用电器研究院","","","新材料","EMI接收机","德国RS公司ESCS30,ESCS30","德国","9k-2750MHz","电磁兼容检测"]
["中国家用电器研究院","","","新材料","三环天线","R&S","德国","","三环天线"]
["中国家用电器研究院","","","新材料","能量色散X荧光光谱仪","纳优科技（北京）有限公司NAU-E610,NAU-E610","国内","","IT,AV类电子产品检测"]
["中国家用电器研究院","","","新材料","红外光谱仪","赛默飞世尔科技（中国）有限公司Nicolet6700,Nicolet6700","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","多功能校准器","美国福禄克公司5500A240,5500A240","美国","","家电附件产品检测"]
["中国家用电器研究院","","","新材料","多功能校准器","美国福禄克公司5700A,5700A","美国","","家电附件产品检测"]
["中国家用电器研究院","","","新材料","导热系数测试仪","美国ANTER公司2031-CBI,2031-CBI","美国","","检测设备的计量与校准"]
["中国家用电器研究院","","","新材料","电热水器产品安全实验室","青岛科通高技术公司","国内","","家电附件产品检测"]
["中国家用电器研究院","","","新材料","单相短路试验系统","苏州安泰变压器有限公司100-5000A,100-5000A","国内","","六种有毒有害物质检测"]
["中国家用电器研究院","","","新材料","臭氧老化试验箱","东莞常平锐铧电子仪器厂yh-8733,yh-8733","国内","","家电附件产品检测"]
["中国家用电器研究院","","","新材料","三相负载柜","东莞越铧设备公司yh-8817te,yh-8817te","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","电机试验测试系统","台州市光中电器制造有限公司MTS-IV-1313,MTS-IV-1313","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","谐波与闪烁测试系统","北京特测电子仪器有限公司profline2105,profline2105","国内","0-40次谐波单相≤18.5A","电磁兼容检测"]
["中国家用电器研究院","","","新材料","NSG3040多功能抗扰度测试仪","北京特测电子仪器有限公司nsg3040,nsg3040","国内","85V-265V50Hz/60Hz","电磁兼容检测"]
["中国家用电器研究院","","","新材料","磁滞测功机","杭州威格智能仪器研究所djc-1,djc-1","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","超高温试验箱","爱斯佩克环境仪器（上海）公司北京分公司STPH-202M,STPH-202M","国内","0-500℃","家电附件产品检测"]
["中国家用电器研究院","","","新材料","耐氢氟酸系统","赛默飞世尔科技（中国）有限公司","国内","","六种有毒有害物质检测"]
["中国家用电器研究院","","","新材料","5匹带工况调节精密级消声室","中国家用电器研究院","国内","","压缩机产品检测"]
["中国家用电器研究院","","","新材料","低温调温调湿试验箱","上海爱斯佩克环境设备有限公司SETN-Z-80ILP,SETN-Z-80ILP","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","灼热丝试验台","TESTING公司T4-08,T4-08","国内","0-960℃","家电附件产品检测"]
["中国家用电器研究院","","","新材料","量规","北京精鑫伟业科技发展中心7006,7006","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","电冰箱性能试验室","中国家用电器研究院","国内","","小家电器具检测"]
["中国家用电器研究院","","","新材料","偶合器量规","北京东山玉机械加工有限公司60320-1/2,60320-1/2","国内","","家电附件产品检测"]
["中国家用电器研究院","","","新材料","冷水机组及多联体空调综合试验","中国家用电器研究院","国内","","制冷器具检测"]
["中国家用电器研究院","","","新材料","电机型式试验自动测试系统","杭州威格智能仪器研究所DJC-14A,DJC-14A","国内","","灯具产品检测"]
["中国家用电器研究院","","","新材料","电动振动试验系统","苏州试验仪器总厂DS-300-2-04,DS-300-2-04","国内","","压缩机产品检测"]
["中国家用电器研究院","","","新材料","压缩机非正常试验装置","自制","国内","","压缩机产品检测"]
["中国家用电器研究院","","","新材料","电容器测试与寿命试验台","CLD-100,CLD-100","国内","0-1200V","家电附件产品检测"]
["中国家用电器研究院","","","新材料","焓差法家用空调器试验台","上海理工大学","国内","","制冷器具检测"]
["中国家用电器研究院","","","新材料","空调器压缩机制冷量测试装置","美国VISTA公司","美国","","压缩机产品检测"]
["中国家用电器研究院","","","新材料","平衡环境型房间型量热计","美国ETL试验室","美国","（1.6～7.1）kW","制冷器具检测"]
["中国家用电器研究院","","","新材料","风扇风量测试系统","自制","国内","","小家电器具检测"]
["中国家用电器研究院","","","新材料","微生物培养洁净室","","国内","","清洁器具检测"]
["中国家用电器研究院","","","新材料","空气净化器性能实验室","北京金亿添成净化科技发展有限公司","国内","","清洁器具检测"]
["中国家用电器研究院","","","新材料","洗衣机,洗碗机性能试验室","工程部","国内","","清洁器具检测"]
["中国家用电器研究院","","","新材料","洗衣机,洗碗机性能试验室","工程部","国内","","清洁器具检测"]
["中国家用电器研究院","","","新材料","十万级微生物实验室","北京金亿添成净化科技发展有限公司","国内","洁净度：≥0.5μm颗粒物浓度<352000个/m3<> 沉降菌：≤3个/皿<> 压差：相邻房间相对静压差≥5Pa，相对室外静压差≥10Pa","检测抗菌、除菌类家电产品 符合GB21551系列标准要求"]
["中国家用电器研究院","","","新材料","30m3空气净化器试验舱","北京金亿添成净化科技发展有限公司","国内","洁净恒温恒湿空调机组：冷量6kW 电热加湿5kg/h<> 中效送风机组：1800m3/h<> 排风机组:1000m3/h<> 循环轴流风机:21.5m3/h<> 高效过滤器:630*630*220","检测空气净化器性能指标 符合GB/T 18801-2008"]
["中国家用电器研究院","","","新材料","洗衣机及清洁器具性能试验室","中加智锐","国内","",""]
["中国家用电器研究院","","","新材料","洗衣机及清洁器具性能试验室","综合检验部","国内","6工位能效水效测试试验台、数字化白度测试系统、参比洗衣机","检测电动洗衣机能效水效限定值及等级 符合GB 12021.4-2013、GB/T 4288-2008"]
["中国家用电器研究院","","","新材料","工频磁场测试系统","特侧","","交/直流、单/三相设备，最大连续电流32A；频率范围DC～500Hz；最大连续磁场1000A/m,最大短时磁场1600A/m；线圈1m×1m；",""]
["中国家用电器研究院","","","新材料","屏蔽室","ETS","","尺寸：9m×5m×3.5m；AC：电压0～400V，频率50Hz～60Hz，单/三相，相电流最大32A；<> DC：电压0～400V，最大电流100A","屏蔽室"]
["中国家用电器研究院","","","新材料","天线","R&S","","频率：9kHz～30MHz；直径：2m","天线"]
["中国家用电器研究院","","","新材料","电磁兼容测试系统","RS/特测","","辐射骚扰测试系统辐射抗扰测试系统：测试频率覆盖范围9kHz～7GHz，场强18V/m；<> 天线升降高度范围：1～4m；<> 转台直径2m,承重2吨","电磁兼容测试系统"]
["中国家用电器研究院","","","新材料","3m法半电波暗室","嘉善法兰克尼亚电磁兼容 有限公司","","尺寸：9m×6m×6m；AC：电压0～400V，频率50Hz～60Hz，单/三相，相电流最大100A；<> DC：电压0～400V，最大电流100A","3m法半电波暗室"]
["中国家用电器研究院","","","新材料","摆管淋雨试验装置","锐铧","国内","可测试IPX1-IPX6防水试验","摆管淋雨试验装置"]
["中国家用电器研究院","","","新材料","噪声振动测试分析系统","中加智锐","国内","两套系统，分别为8通道和12通道，可测试噪声和振动试验","噪声振动测试分析系统"]
["中国家用电器研究院","","","新材料","冰箱压缩机性能试验台","中加智锐","国内","","冰箱压缩机性能试验台"]
["中国家用电器研究院","","","新材料","电动机-压缩机堵转试验装置","中加智锐","国内","可测试堵转电流0-150A的压缩机","电动机-压缩机堵转试验装置"]
["中国家用电器研究院","","","新材料","空调压缩机非正常试验装置","中加智锐","国内","可测试输入功率3000W-8000W的压缩机","空调压缩机非正常试验装置"]
["中国家用电器研究院","","","新材料","冰箱压缩机非正常试验装置","中加智锐","国内","可测试输入功率50W-500W的压缩机","冰箱压缩机非正常试验装置"]
["中国家用电器研究院","","","新材料","房间空调压缩机性能试验台","大西热学","国内","可测试制冷量1000W-18000W的压缩机","房间空调压缩机性能试验台"]
["中国家用电器研究院","","","新材料","声学实验室","院噪声课题组","国内","室内侧房间：5.0 * 4.4 * 4.0M<> 室外侧房间：5.0 * 6.0 * 4.0M<> 工况机组功率最大：5匹","声学实验室"]
["中国家用电器研究院","","","新材料","潮态室","中加智锐","国内","温度：环温——50℃<> 湿度：30%——95%RH","潮态室"]
["中国家用电器研究院","","","新材料","空调压缩机耐久性试验台","中加智锐","国内","可测试输入功率在600W——6000W内的压缩机，4工位","空调压缩机耐久性试验台"]
["中国家用电器研究院","","","新材料","电动机-压缩机机械强度试验装置","中加智锐","国内","可测试0-60MPa的压力试验","电动机-压缩机机械强度试验装置"]
["中国家用电器研究院","","","新材料","毛细管堵塞率试验台","中加智锐","国内","可测试输入功率在0W——500W内的R134a制冷剂的压缩机","毛细管堵塞率试验台"]
["中国家用电器研究院","","","新材料","单相短路试验系统","苏州安泰变压器厂","国内","0—5000A","单相短路试验系统"]
["中国家用电器研究院","","","新材料","开关寿命试验台","东莞锐铧","国内","操动行程0.1～100mm，操动速度0.1～300mm/s",""]
["中国家用电器研究院","","","新材料","控制器寿命耐久性试验装置","青岛科通","国内","突跳式、双金属片式",""]
["中国家用电器研究院","","","新材料","电容器测试与寿命 测试台","广州微仪电子","国内","试验电压输出0-700V，电容器容量：5-100μF",""]
["中国家用电器研究院","","","新材料","电热水器产品安全、性能综合检测实验室","青岛科通","国内","环境温度：（0-50）℃；环境湿度：（0-100）%RH；热电偶：（0-200）℃；进水压力：（0-10）bar",""]
["中国家用电器研究院","","","新材料","A、C型换气扇空气性能","广州市先河技术工程有限公司","国内","--",""]
["中国家用电器研究院","","","新材料","吸油烟机空气性能试验装置","中加智锐","国内","最大静压重复性：0.54%；???? 风量准确度：-1%；??????????? 风量重复性：0.22%。",""]
["中国家用电器研究院","","","新材料","吸油烟机油脂分离度验装置","中加智锐","国内","压力控制：-50Pa-100Pa；电炉功率：1800W",""]
["中国家用电器研究院","","","新材料","电风扇性能实验室","广州市先河技术工程有限公司","国内","电压：（0-300）V；电流：（0-10)A；功率：（0-3000）W；",""]
["中国家用电器研究院","","","新材料","吸油烟机气味降低度试验装置","青岛科通","国内","",""]
["中国家用电器研究院","","","新材料","室内加热器环境 实验室","青岛科通","国内","黑球温度：（0-40）℃；热电偶（0-100）℃；电压（0-600）V；功率：（0-3000)W；温场：-40℃-30℃",""]
["中国家用电器研究院","","","新材料","外排式吸油烟机风量测试装置","中家智锐","国内","最大静压重复性：0.54%；???? 风量准确度：-1%；??????????? 风量重复性：0.22%。",""]
["中国家用电器研究院","","","新材料","风冷型、水冷型冷水（热泵）机组综合性能试验装置<> 及多联体空调焓差测试装置（30P焓差）","中加智锐","国内","2.5-90kW（冷风机组）<> 5.0-60kW（冷水机组）<> 单元机40kW以下室外具有复测功能<> 5.0-60kW（多联机）<> 水温（5-50℃±0.1℃）<> 风冷（-10-55℃，相对湿度45-90%）<> C室250-210m3/h<> B1 2500-6000m3/h<> B2 2500-10000m3/h<> A室 同B1???????????????????? A室： 9000（W）×7500（D）× 4300（H）<> B室：9000（W）×7500（D）×4300（H）<> C室：5400（W）×4500（D）×3200（H）","检测压缩机、热泵热水器空调性能与功率"]
["中国家用电器研究院","","","新材料","5HP房间空调器焓差法试验室","中加智锐","国内","1.2-14kW（制冷）<> 1.4-16kW（制热）<> 风量：300-2100内：W5.5×D4.5×H3.2<> 外：W4.5×D4.5×H3.2","检测空调的安全性能与能耗"]
["中国家用电器研究院","","","新材料","家用制冷器具性能实验室","中加智锐","国内","6工位<> （10℃-43℃,±0.3℃/45%-95%，±3%/50-300V/0-20A）","检测家用制冷电器的安全与性能功率"]
["中国家用电器研究院","","","新材料","空调平衡式房间型量热计","大西热学","国内","1.2-13kW（制冷）<> 1.2-14kW（制热）","检测空调的制冷制热量"]
["中国家用电器研究院","","","新材料","电冰箱可燃性制冷剂泄漏模拟装置","中家智锐","国内","测量范围（0-50）℃","测量制冷剂的泄漏量"]
["中国家用电器研究院","","","新材料","空调器制冷系统承压寿命试验装置","中家智锐","国内","1.2-13kW","检测空调制冷系统的寿命"]
["中国家用电器研究院","","","新材料","冰箱环境试验室","中家智锐","国内","120℃，98%","测量电器的性能、负载温度回升、安全性能、好电量"]
["中国家用电器研究院","","","新材料","冷柜型式试验室","中加智锐","国内","（10-43）℃","测量电器的性能、负载温度回升、安全性能、好电量"]
["中国家用电器研究院","","","新材料","洗衣机安全实验室(加3个电热水器测试工位，报价含在此）","中家智锐","国内","电流量程0-40A，电压220V、水压范围0.1-1MPa","检测家用清洁器具的安全性能、功率"]
["中国家用电器研究院","","","新材料","洗衣机性能实验室","中家智锐","国内","电流量程0-40A，电压220V,冷热水箱10-70℃可调","检测家用清洁器具的安全性能、功率"]
["中国家用电器研究院","","","新材料","空调环境试验室(空调5P焓差试验室)","中家智锐","国内","1.2-14kW（制冷）<> 1.4-16kW（制热）<> 风量：300-2100内：W5.5×D4.5×H3.2<> 外：W4.5×D4.5×H3.2","检测空调的安全性能与能耗"]
["中国家用电器研究院","","","新材料","冰箱开门机（含洗衣机开门机功能）","中家智锐","国内","功率（20-25）次/分","检测洗衣机、冰箱的功率级能效值"]
["中国家用电器研究院","","","新材料","电冰箱制冷系统易触及表面刮擦试验装置","中家智锐","国内","--","检测易触面刮擦承受度"]
["中国家用电器研究院","","","新材料","人工环境试验室（湿热试验室）","中家智锐","国内","温度：环温——50℃<> 湿度：30%——95%RH","检测家用电器耐潮湿试验符合GB 4706.1"]
["中国家用电器研究院","","","新材料","电磁兼容测试系统（EMScan）","EMSCAN? FSL3","加拿大","--",""]
["中国家用电器研究院","","","新材料","太阳能热水器系统是一整套东西","中家智锐","国内","温度：-40℃～150℃（PTWD-2A）-40℃～300℃（PTWD-1A）环境温度: -40℃～70℃<> 风速: 0～60m/s<> 太阳辐射: 0～2000W/㎡<> 流量: 0.2～1.2m3/h<> 环境温度: -40℃～70℃<> 风速: 0～60m/s<> 太阳辐射: 0～2000W/㎡<> 流量: 0.2～1.2m3/h<> <>","检测家用太阳能热水器能效限定值和能效等级 符合GB26969-2011、GB/T 19141-2011、GB/T 18708-2002"]
["中国家用电器研究院","无","无","新材料","SR954","容向","国内","屏蔽室，8.7m×5.2m×3.6m，气动屏蔽门尺寸1.5×2.0m","测试环境"]
["中国家用电器研究院","无","无","新材料","Nicolet 6700","赛默飞世尔","国内","红外光谱仪（含红外灯、热膜压仪）","红外光谱仪"]
["中国家用电器研究院","无","无","新材料","TG 209F3","耐驰","德国","热重分析仪（带自动进样器）","差示扫描量热仪及热重分析仪"]
["中国家用电器研究院","无","无","新材料","DSC 200F3","耐驰","德国","差示扫描量热仪（带自动进样器）","差示扫描量热仪及热重分析仪"]
["中国家用电器研究院","无","无","新材料","NSG 4070-75","TESEQ","德国","射频传导抗饶度测试系统主机，内置9kHz -1GHz信号源，支持1Hz -50kHz 幅度调制AM，调制深度0%-100%可调，以及脉冲调制。内置三通道9kHz -1GHz功率计，以及150kHz -230MHz 功率放大器模块，最小1dB输出线性功率75W，包括免费远程控制软件","射频传导抗扰度测试系统,IEC 61000-4-6"]
["中国家用电器研究院","无","无","新材料","NSG 3040-IEC","TESEQ","德国","多功能瞬态抗扰度测试仪, 符合EN/IEC 61000-4-4,5,11,29标准。雷击浪涌1.2/50-8/20us混合波，最高电压4.4kV，快速瞬变脉冲群，5ns/50ns波形，最高电压4.8kV，脉冲频率100Hz -1MHz，交直流两用电压跌落与中断，内置单相260Vac/dc，16Aac/dc电源线耦合去耦网络","瞬态抗扰度测试系统,IEC 61000-4-4/5/11"]
["中国家用电器研究院","无","无","新材料","DPA500N","EMTEST","瑞士","单相谐波闪烁分析仪，含16A闪烁阻抗及控制软件 dpa.control","谐波闪烁测试系统"]
["中国家用电器研究院","无","无","新材料","Netware 7","EMTEST","瑞士","单相多功能AD/DC电源，7.5kVA，含任意波形发生器，符合IEC 61000-4-13, -4-14, -4-17, -4-28, -4-29标准","谐波闪烁测试系统"]
["中国家用电器研究院","无","无","新材料","CL 55C","AFJ","意大利","喀呖声分析仪，全兼容CISPR 16-1-1和CISPR 14-1，4个固定频率模块（频率为150 kHz，500 kHz，1.4 MHz，30MHz），可同时测量，内置脉冲信号发生器。含分析软件","断续骚扰（喀呖声）测试系统"]
["中国家用电器研究院","无","无","新材料","EMC32","R&S","德国","EMI测量软件","EMI测试系统，符合CISPR 14-1，CISPR 15以及CISPR 11"]
["中国家用电器研究院","无","无","新材料","ESCI","R&S","德国","EMI全兼容测试接收机，频率范围9kHz-3GHz，含 ZZA-478和ESCI-DCV","EMI测试系统，符合CISPR 14-1，CISPR 15以及CISPR 11"]
["中国家用电器研究院","无","无","新材料","微生物培养洁净室Y11-S-09-B","","国内","",""]
["中国家用电器研究院","无","无","新材料","空气净化器性能实验室Y11-S-09-A","北京金亿添成净化科技发展有限公司","国内","",""]
["中国家用电器研究院","无","无","新材料","洗衣机,洗碗机性能试验室Y09-S-07(B)","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","洗衣机,洗碗机性能试验室Y09-S-07(A)","综合检验部","国内","",""]
["中国家用电器研究院","无","无","新材料","工频磁场抗扰度设备","特侧","","",""]
["中国家用电器研究院","无","无","新材料","屏蔽室","ETS","","",""]
["中国家用电器研究院","无","无","新材料","三环天线","R&S","","",""]
["中国家用电器研究院","无","无","新材料","暗室配套设备","RS/特测","","",""]
["中国家用电器研究院","无","无","新材料","半波暗室","嘉善法兰克尼亚电磁兼容有限公司","","",""]
["中国家用电器研究院","无","无","新材料","摆管淋雨试验系统","锐铧","国内","",""]
["中国家用电器研究院","无","无","新材料","噪声测试设备","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","冰箱压缩机量热计","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","5匹工况调节精密级半消声室","院噪声课题组","国内","",""]
["中国家用电器研究院","无","无","新材料","人工气候环境试验室Y11-S-10","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","空调压缩机寿命,停开（4工位）Y11-S-11","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","压缩机耐压试验装置Y11-S-06","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","R134a冰箱压缩机毛细管堵塞试验台Y11-S-05","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","压缩机堵转试验台及控制系统Y11-S-04","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","空调压缩机非正常试验装置Y09-S-06","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","冰箱压缩机非正常试验台Y09-S-05","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","空调压缩机量热计","大西热学","国内","",""]
["中国家用电器研究院","无","无","新材料","分断系统(一期?限定短路\n实验装置)","苏州安泰变压器厂","国内","",""]
["中国家用电器研究院","无","无","新材料","开关耐久性试验装置","东莞锐铧","国内","",""]
["中国家用电器研究院","无","无","新材料","控制器类产品耐久性试验台","青岛科通","国内","",""]
["中国家用电器研究院","无","无","新材料","电容器测试台","广州微仪电子","国内","",""]
["中国家用电器研究院","无","无","新材料","台、吊扇试验室","广州市先河技术工程有限公司","国内","",""]
["中国家用电器研究院","无","无","新材料","吸油烟机气味降低度试验装置","青岛科通","国内","",""]
["中国家用电器研究院","无","无","新材料","室内加热器试验室","青岛科通","国内","",""]
["中国家用电器研究院","无","无","新材料","热水器性能试验室","青岛科通","国内","",""]
["中国家用电器研究院","无","无","新材料","换气扇性能试验室(A、C型)","广州市先河技术工程有限公司","国内","",""]
["中国家用电器研究院","无","无","新材料","吸油烟机空气性能试验装置(B型)Y11-S-03","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","吸油烟机油脂分离度试验装置Y11-S-02","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","脉冲压力测试仪（5MPa）Y11-S-08","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","可燃制冷剂模拟泄漏装置(自动控制)Y11-S-07","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","洗衣机安全试验台（8台位）Y11-S-01","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","30HP焓差空调测试室Y09-S-04","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","5HP空调焓差试验室Y09-S-03","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","食品冷柜型式试验室Y09-S-02","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","冰箱性能试验室Y09-S-01","中加智锐","国内","",""]
["中国家用电器研究院","无","无","新材料","3HP空调热平衡试验室","大西热学","国内","",""]
["中国家用电器研究院","无","无","新材料","5HP空调焓差试验室","大西热学","国内","",""]
["中国家用电器研究院","无","无","新材料","六台位冰箱试验室","佐竹冷热","国内","",""]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}